**

**AMERICAN ACADEMY ALUMNI FOUNDATION**

(A Corporation Limited by Guarantee and founded in 1973)

32 Gregory Afxentiou Avenue,

P.O. Box 40112, 6301 Larnaca, Cyprus

Telephone No: 24815400

Telefax: 24651046

e-mail: info@academy.ac.cy

[www.academy.ac.cy](http://www.academy.ac.cy)

**Monday, February 24, 2025**

Supply and installation of a Theatre projector and motorized screen at the American Academy Larnaca (private school) premises

# Introduction

The American Academy Alumni Foundation (AAAF) owner of the American Academy Larnaca is looking to appoint a contractor for:

1. The supply and installation of a theater projector and motorized screen as described on table “A”.
2. Tenders should be valid until **24th of April 2025.**
3. The successful tenderer must be able to complete the works by **1/06/2025**

# Procedures

The successful tenderer will be expected to:

1. To carry out ALL of the required work according to the health and safety regulations of the department of labor and inspection.
2. To provide ALL of the certificates (as may be required by Cyprus legislation) for the type/specifications/approval of service/product
3. To complete ALL of the fields as outlined on the **TABLE “A”** at the tender submission page 3.

# Placement of offers

1. Tenders should be submitted in a sealed envelope by **12:00 a.m., on Thursday 13thof March 2025** in the Tender Box of the Treasury Office (Graduates Centre Building / Markou Drakou street, Larnaca).
2. **Incomplete tenders will be excluded.**
3. **The AAAF is not obliged to accept the lowest or any tender.**
4. **If any clarifications needed please contact Mr. Antonis Constantinou 99439395 or Mr. George Gavriel 99455350**

**AMERICAN ACADEMY ALUMNI FOUNDATION**

**TENDER SUBMISSION PAGE (page 3)**

**TABLE A:**

|  |  |  |  |
| --- | --- | --- | --- |
| **ITEM (SHORT DESCRIPTION)** | **QUANTITY** | **UNIT PRICE in euro (€)** | **TOTAL PRICE in euro (€)** |
| **Projector**  |
| **Color/White Brightness:** at least 6,000 lumens **Native Resolution:** Minimum WUXGA **Contrast Ratio**: 2,500,000:1 | 1 |  |  |
| **Connectivity:** HDMI and VGA |  |  |  |
| **Distance:** around 4 meters from screen |  |  |  |
| Projector needs to cover fully the screen surface below. |  |  |  |
|  |  |  |  |
| **Motorized Screen** |  |  |  |
| **Size:** minimum 700cm,height >500cm. Motorized screen. Background color white or gray. Ceiling mounted | 1 |  |  |
|  |  |  |  |
| Installation and other related |  |  |  |
| ALL other costs (please outline) |  |  |  |
|  |
| TOTAL |  |  |  |
| VAT |  |  |  |
| GRAND TOTAL |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

|  |
| --- |
| Company Name: |
| Authorized Person’s Name: |
| Signature: |
| Date: |
| Contact telephone/mobile no: | Email address: |